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The loudspeaker shall be a passive two-way rear-ported bass-reflex system. The transducers shall be a 12-inch (305-millimeter) ferrite woofer and a titanium-diaphragm neodymium compression driver with 2-inch (51-millimeter) voice coil. The loudspeaker shall use a passive internal crossover at 2.7 kHz. 
The loudspeaker shall meet the following performance specifications. The on-axis system frequency range shall be 45 Hz to 20 kHz (-10 dB) with the use of recommended active equalization. The sensitivity shall be 98 dB SPL in a whole-space environment with recommended high-pass protection with 1 watt input at 1 meter. The long-term continuous power handling rating shall be 600 watts (AES test methodology using pink noise filtered to meet IEC 268-5 with a 6-dB crest factor for 2 hours). The maximum continuous output shall be 126 dB SPL, and the maximum peak output shall be 132 dB SPL. The nominal rated impedance shall be 8 ohms. The nominal coverage pattern shall be 90 degrees horizontal by 60 degrees vertical with a rotatable high-frequency waveguide behind a removable grille. 
The loudspeaker enclosure shall be constructed of plywood, 15 millimeters (0.6 inches) thick, with a black polyurethane coating. The transducers shall be located behind a perforated steel grille with a black, powder-coated finish. The loudspeaker shall be suitable for indoor use only. The input connectors shall be two Neutrik speakON NL4MP connectors. The loudspeaker shall include three M8 threaded inserts on the top panel and four M8 threaded inserts on the side panel for suspension. The loudspeaker shall include three M8 threaded inserts on the bottom panel for attachment to an optional external pole adapter to mount the loudspeaker on a standard 35-millimeter (1.4-inch) loudspeaker pole. The loudspeaker shall include four M8 threaded inserts on the rear panel for attachment to an optional bracket. 
The dimensions of the loudspeaker shall be 600 millimeters (23.6 inches) in height, 360 millimeters (14.2 inches) in width, and 420 millimeters (16.5 inches) in depth. The net weight of the loudspeaker shall be 23.1 kilograms (50.9 pounds). 
The loudspeaker shall be the ShowTime SK12 loudspeaker.

