INSTRUCTIONS FOR MANUALLY INSTALLING FORUM SPM FILES FOR MODELER APPLICATION:


Locate your Modeler installation path. Typically, this should be something like
	C:\Program Files (x86)\Bose\Bose Modeler 6.11

Go to ...\data\speaker_data\Bose
	you should now see subfolders for the various product series

Copy the DML88P.bmp file into the '\Images' folder.

Copy the DML88P.spm files (3) into the '\DesignMax\Pendant' folder.


NOTES FOR USING THE DML88P SPM FILES:

The DML88P spm files are low-impedance and CV passive versions including the recommended speaker EQ.


As usual, the SPM speaker data is defined for Continuous (LEQ/RMS) SPL. For DM speakers, assuming sufficient peak power is available from the selected amplifier, Peak SPL up to 6 dB higher than RMS SPL can be expected (without considering power compression). As an example, if you want to predict maximum LEQ SPL for a signal with 12 dB crest factor, you need to subtract 12-6 = 6 dB from the predicted SPL. 
For CV amplifiers, depending on limiter settings, the available peak power may only be 3 dB higher than the RMS power, changing the above correction from -6 to -9 dB.


Rev 2025-09-29